**Model 3448 Comfort Station**

Dimensions 34” Wide x 48” Long 81” High

Custom Dimensions Available

(Patents Issued and Pending)

Model 3448 also eliminates the need to construct bathrooms for your employees and then dismantle them to build the bathrooms for your customers.

A close up of a door

Description automatically generatedA picture containing wall, indoor, bathroom

Description automatically generated

Exterior Front View Top Interior View Rear Exterior View

**Rear Wall Plumbed Attachments**

**A wooden box

Description automatically generated A picture containing object, wall, toilet, indoor

Description automatically generated A picture containing indoor, wall, table, yellow

Description automatically generated** A picture containing indoor, object, wall, floor

Description automatically generated

**18” Vanity Waterless Urinal Eye Wash Hand Wash**

**Hand Sanitizer Station Station**

Model 3448 comfort station was specifically developed for multistory construction projects that have size restrictions. The units can be loaded on their side in the freight elevator.

**Standard Features**

Ceramic Toilet and Sink Combination – 9” Toilet Tissue Dispenser **–** Paper Towel Dispenser – Mirror – Waste Basket – Supply of Consumables – Heavy Duty Door With Indicator Usage Lock - Aluminum Corners – ½” Fluted FRP Sheet Pebbled on Both Sides and Graffiti Resistant – Treated Wood Runners – Treated Plywood Floor – Coin Vinyl Flooring – Mobility Via a Pallet Jack –

Foaming Hand Soap Dispenser – Aluminum Door Jamb – Stainless Steel Door Hinges – Smoke Detector – Double Clamshell Door

The Model 3448 is manufactured to be used on multiple projects with minimal maintenance required.

A bathroom with a sink and a mirror

Description automatically generated A picture containing indoor, wall

Description automatically generated

Multiple Model 3448 Views Walls can be used

for Signage

**Options:**

Model 3448 ships without a roof. Special attention will be paid to the height restrictions of the freight elevator on multiple story or underground projects. The 3448 height can be adjusted, or the unit can be tipped on its back.

**Toilet and Sink and Faucet Choices**

We offer several handwash system choices for the Model 3448 comfort station.

**A picture containing indoor, object, floor, toilet

Description automatically generatedA white sink sitting under a mirror

Description automatically generated**

**Fig 1. Fig. 2**

Standard P-trap Toilet (above Fig 1.) and rear wall outside vanity (above Fig 2.) Vanity ships inside the Model 3448. The unit can be plumbed to the live water and sewer lines.

Cistern-Sink-Toilet Combination inside the Model 3448 allows us to custom design sanitation for most requirements.

A picture containing floor, indoor, toilet, object

Description automatically generated A picture containing indoor, refrigerator, sitting, kitchen

Description automatically generated A bathroom with a white door

Description automatically generated

Combination Hand Sanitizer Front View of

Cistern and Sink Stand/Storage Model 3448